Step 1:  Sort and layout all lift hardware.

Major Lift Components: 

NOTE IF YOU ORDERED OPTIONS THEY ARE NOT INCLUDED:

3000lb thru 20,000lb (4) post:

  (2) IBEAMS WITH ENDS
  (2) TOP UNITS COMPLETE
  (2) MOTORS WITH DRIVE UNITS, BELTS AND PULLEYS AND SWITCH
  (2) BOARDS CARPETED
  (4) CABLES
  (4) PULLEYS
  (4) AXLE BOLTS AND NUTS
  (4) CABLE CLAMPS
  (8) PRE ASSEMBLED BUNK BRACKETS (2" X 2" ANGLE)
  (4) PRE ASSEMBLED GUIDE POST BRACKETS (2" ROUND TUBE)
  (4) 3' WEIGHT PIPE 1.5" GAL. PIPE
  (4) P.V.C WITH DRILLED CAPS
  (4) CABLE ADJUSTERS WITH HARDWARE
  (2) WHITE COVERS WITH HARDWARE (LABELED IN BAG)
  (4) 1/2" X  1.3/4" HEX BOLTS WITH NYLON NUTS (HOIST PLATE TO LIFT                  
      BOLTS)
  (2) MOTOR SPACERS (2" X 4") ALUMINUM PIPE WITH HOLE)
  (5) RUBBER 10" X 10" RUBBER PADS
 (16) 3/8" HEX BOLTS LABELED BUNK BOLTS
 ( 4) STAINLESS STEEL CABLES
      
16,000LB AND 20,000LB LIFTS ONLY:

( 4) 1/2" x 2 1/2" HEX BOLT AND (2) SQUARE ALUMINUM WASHERS (DEADMAN 
     FOR CABLE)

*NOTE HARDWARE TO MOUNT LIFT TO PILING IS NOT INCLUDED.

REQUIRED TOOLS:
LEVEL
HAMMER
DRILL
3/8" METAL BIT
1/2" AUGER BIT TO DRILL PILINGS
RAZOR KNIFE
(2)  3/4"  WRENCH
(2) 9/16"  WRENCH
(1) 7/16"  WRENCH
(2) 1 1/8" WRENCH
(1) #2  PHILLIPS HEAD SCREW DRIVER