PWC ELECTRIC

(1) TRACK - 3 x 4 I-BEAM

(1) CRADLE ARM (WITH 3” PULLEY)

(1) MOTOR PLATE TO LIFT (2) ¼ X 1 ¼  (4) FLAT WASHER (2) NUTS

(1) CABLE CLAMP

(1) CABLE ¼ X 20’ CABLE WITH LOOPED END

(4) BUNK BRACKETS (4) 2X3X¼ ANGLES (8) 3/8X6/12 BOLTS (4) 1/4X2  
     FLATPLATE 4” (8) 3/8 LOCK WASHERS (8) 3/8 NUTS (4) 3/8X2 ½” BOLTS  
     FLAT WASHER & NUTS

(2) CARPETED BUNK 

(2) WEIGHT PIPES (2) 1 ½ GAL PIPES 3’

(2) GUIDE PIPES (2) 2” PVC PIPES 3’

(1) ZINC

(1) PILING MOUNT OR DOCK MOUNT (2) 3/8X4 ½ BOLTS LOCK NUT & NUTS

(1) MANUAL GEAR UNIT WITH SELF LOCKING BRAKE

OPTIONS:	ALUMINUM BUNK